These D2XX drivers are for Windows CE 4.2 onwards.

DO NOT INSTALL THESE DRIVERS IF YOU WANT THE DEVICE TO APPEAR AS A COM
PORT - INSTALL THE NORMAL VCP DRIVERS INSTEAD.

Drivers are provided for ARM/Scale processors, MIPS II processors, MIPS
IV processors, SH4 processors, and for 32-bit x86 processors.

Drivers for Windows CE 4.2 through to Windows CE 5.2, Windows Mobile 5,
Windows Mobile 6, Windows Mobile 6.1, Windows Mobile 6.5, Windows Mobile
2003, and Windows Mobile 2003 SE are in the "Mobile 5-6, PocketPC 2003,
CE 4.2-5.2" folder.  Within that folder are folders for ARM/XScale
processors, MIPS II processors, MIPS IV processors, SH4 processors,  and
for 32-bit x86 processors.

Drivers for Windows CE 6.0 and Windows CE 7.0 are in the "CE 6.0-7.0"
folder.  Within that folder are folders for ARM/XScale processors, MIPS
II processors, MIPS IV processors, SH4 processors, and for 32-bit x86
processors.  The "3rdParty" sub-folders within the "ARM, XScale" and
"x86" folders contain driver catatog files for CE 6.0 and CE 7.0.  See
"AN_319_Windows_CE_Driver_Catalog_Item_Usage.pdf" for driver catalog
usage.

Drivers for Windows Embedded Compact 2013 are in the "CE 2013" folder.
Within that folder are folders for ARM/XScale processors, and for 32-bit
x86 processors.  This is a "BETA" release.


Note that the USB serial converter needs to be connected to a USB host
port on the device to which it is connected.  Not all PDAs have a USB
host port as standard, but it may be available as an add-on. The regular
USB port used for PC synchronization etc. will not work.
